SendTxWatchdogValue | Top Next

SendTxWatchdogValue send TxWatchdog Counter Value Since R2019b Library: CAN Bus Controller ( Dafulai Electronics) /SendTxWatchdogValue Description This block will set Hardware TxWatchdog counter value for Txwatchdog Mode 0. If TxWatchdog is not enabled, system just ignore this block. Parameters Please double click this block to open parameters dialog below: Let us explain parameters.
• | Object ID for multiple CAN Bus controllers — In one PC, we may use multiple CAN bus controllers, this is for identifying each one we use. It must match the same parameter in CAN_setup block.
Ports Input Din — "number" scalar. Value Range is from 2 bytes of integer. If Counter is one byte, it will only use LSB automatically, Outport None Examples