Example | Top Previous

Examples Example1: Our embedded platform is dsPIC33EP256GP502 . Uart2 connects RS485 Transceiver, and TX_transmit Enable is controlled by RB11. Logic High will enable RS485 transmit and disable RS485 receiver. Our embedded Modbus Server ID=1, and supports discrete registers address range: 10008 to 10025, baud rate=19200 Please see screenshot of model below: In "Setup Target" block, we choose "PIC24/Dspic30/Dspic33" platform. Double click "emModbusServerDebugSetup", we will see the Modbus Server/Debug parameters settings below: In our hardware environment, we use "Modbus RTU/ASCII Dual Masters adaptor" as debugger/monitor. Please plug into "Modbus RTU/ASCII Dual Masters adaptor" to your PC USB Port. And if you are the first time to use this adaptor, run software "ConfigTool.exe" to config debug/monitor tool: In above configuration, The first Uart setting must match Target including baud rate and physical interface (RS485/RS422/RS232). The second part setting can be different, but you must make sure parameter "PC Side USB/Bluetooth Serial Port Baud Rate" in "emModbusServerDebugSetup" block matches it. Double click "emMBSlaveReadDiscretes", we will see the "emMBSlaveReadDiscretes" parameters settings below: It means this block will update discrete register from Modbus server ID=1. This block's in-port "StartAddr" connects Constant block with value= 8 which denotes discrete register starting address is 10008. This block's in-port "Data" connects "Constant" block output, which provide boolean vector [1 1 1 0 0 0 1 1 1 0 0 0 1 1 1 1 1] to in-port "Data". So we will see Modbus server (ID=1) discrete register 10008 to 10010 with value "true", discrete register 10011 to 10013 with value "false", ... , discrete register 10020 to 10024 with value "true". Before you build this simulink model, you must create the firmware project by your IDE. and remember the firmware project directory name. In our example, it is microchip MPLAX IDE software, you must use MCC to configure timer1 as 1ms timer and interrupt enabled. You must use MCC to enable Uart2 with interrupt enabled and both "software Transmit Buffer Size" and "software Receive Buffer Size" =255 or 254. Timer1 interrupt priority is below UART (you can choose equal too). We put our MCC configuration file BasePrj.mc3 into example folder for your reference. You must modify according to your hardware. You'd better compile your firmware which is created by MCC to identify any error by MCC. After your "Modbus RTU/ASCII Dual Masters adaptor" connects to Target (dspic33) and PC USB, right click on any empty space of simulink model, pop up context menu, click on menu item "Build Embedded Target and open its IDE" It will start build, and popup dialog window to input base sampling period: Input your base sample time and click OK. If any error occurs, it will stop building, and display error information. The error block will display in Yellow color. If build successfully, it will popup window to ask you firmware directory for your IDE project. If you give out the correct IDE project directory, Simulink will open IDE software automatically. And you can compile firmware in your IDE, and program into Target by emulator IDE supported. If your firmware program into target successfully, you can use ModScan32 software to view result below: All results are what we expect. Disconnect ModScan32 software, we can use Simulink directly view results. By select stop time= inf, and click "Run" button, you will see result below: You will see all results in all "Display" Blocks. Notes: You can run both ".ModScan32 " and "Simulink" at the same time. But you must enable "Modbus RTU/ASCII Dual Masters adaptor" Bluetooth, .and "ModScan32" cannot use the same COM port as Simulink. We recommend to use Simulink instead of ".ModScan32 " because " ModScan32 " cannot watch general variables. Simulink can watch any variables by "Probe" (also called emProbe) blocks. Please open "Your embedded creator library folder"/examples/example3_emReadDiscretes.slx (You must change "PC Com Port for Debug or Monitor" in emModbusServerDebugSetup block according to your physical USB port number)