emSPI_I2CAllDone | Top Next

emSPI_I2CAllDone embedded SPI/I2C bus all sequences Done? Since R2019b Library: embeddedCreatorLib ( Dafulai Electronics) / Embedded SPI/I2C Bus Master / emSPI_I2CAllDone Description This block is used in judgment whether all sequences finish for SPI/I2C operation. In order to start a new group of sequences operations, you must set bus into "Idle" state when all sequences done. Parameters Please double click this block to open parameters dialog below: Let us explain parameters.
• | Peripheral Number — tell system which SPI/I2C peripheral is used. You just choose from drop list items which are from block "emSPI_I2CMasterSetup".
• | Bus Type — tell system which bus is used. You just choose from drop list items: SPI bus and I2C bus.
• | Sample time in sec (-1 for inherited): — Sample time for this block. It is the same meaning as general Simulink block .
Ports Input None Outport
• | Yes — "logical" data type's scalar. True means all sequences done.
Examples