emCANChannelAllTxDone | Top Next

emCANChannelAllTxDone emCAN bus all transmission sequences Done? Since R2019b Library: embeddedCreatorLib ( Dafulai Electronics) / Embedded CAN Bus / emCANChannelAllTxDone Description This block is used in judgment whether all sequences finish for CAN bus one transmission channel. In order to start new transmission operations, you must set transmission channel into "Idle" state when all sequences done. Parameters Please double click this block to open parameters dialog below: Let us explain parameters.
• | Peripheral CAN bus Number — tell system this block is which CAN controller peripheral used. You just choose from drop list items: 1 or 2.
• | Transmit Channel: — drop list to select transmission Channel A or Channel B or Channel C.
• | Sample time in sec (-1 for inherited): — Sample time for this block. It is the same meaning as general Simulink block .
Ports Input None Outport
• | Yes — "logical" data type's scalar. True means all sequences of this transmission channel done.
Examples