setMB2Idle | Top Next

setMB2Idle Set embedded Modbus Master to Idle state Since R2019b Library: embeddedCreatorLib ( Dafulai Electronics) / Embedded Modbus Master / setMB2Idle Description This block sets up Modbus master to "Idle" State. You must call it under condition: modbus master all reading/writing operations done. Otherwise, you will get unexpected result. Only when Modbus master is in "Idle" state, can you start new operations for modbus master to read/write server registers. Parameters None Ports Input
• | En — "logical" data type's scalar. True means " it sets Modbus master to idle state". False means nothing happens.
Outport
• | Success — "logical" data type's scalar. It is equal to "En".
Examples