Dout | Top Next

Dout Digital output Since R2019b Library: embeddedCreatorLib ( Dafulai Electronics) / Dout Description This block sets digital output. Parameters Please double click this block to open parameters dialog below : Let us explain parameters.
• | How to specify Digital Output — radio selection button for Digital output Pin. It can be one of "By physical port name and bit number"/"By C language writing variable/macro name".
• | Port Name — drop list for Digital Port name. It is used only when parameter "How to specify Digital Output" is "By physical port name and bit number".
• | Port Bit number — drop list for Digital Port Bit Number. It is used only when parameter "How to specify Digital Output" is "By physical port name and bit number".
• | C Access Variable/Macro Name — String type of scalar. It can be variable name or macro name in C language for Digital output. It is used only when parameter "How to specify Digital Output" is "By C language writing variable/macro name".
• | Initial Output Value: — Logical type of scalar. It is initial value for "Digital Output".
• | Sample time in sec (-1 for inherited): — Sample time for this block. It is the same meaning as general Simulink block .
Notes: Please configure GPIO. All settings must be done in IDE GUI configuration (It is MCC for Microchip Micro-controller). And it must match this block settings, otherwise unexpected result will occur. Ports Input
• | Dout — Logical Scalar. Digital output Value.
Outport None Examples