Example | Top Previous

Examples Example1: SPI bus access. Our embedded platform is dsPIC33EP256GP502 . Please see MCC configuration for SPI bus below: Please see screenshot of model below: Please open "Your embedded creator library folder"/examples/example12_emSPI.slx (You must change "PC Com Port for Debug or Monitor" in emModbusServerDebugSetup block according to your physical USB port number) Example2: I2C bus access Our embedded platform is dsPIC33EP256GP502 . Please see MCC configuration for I2C bus below: Please see screenshot of model below: Please open "Your embedded creator library folder"/examples/example13_emI2C.slx (You must change "PC Com Port for Debug or Monitor" in emModbusServerDebugSetup block according to your physical USB port number)