simEEPROMWrite | Top Next

simEEPROMWrite Write simulated EEPROM Since R2020b Library: embeddedCreatorLib ( Dafulai Electronics) / Simulate EEPROM by Flash / simEEPROMWrite Description This block write "Simulated EEPROM". Actually it only write to "SRAM", it didn't write to "Flash". You must call block "simEEPROMWriteFlash" to do actual writing to flash before power off. Parameters
• | Sample time in sec (-1 for inherited): — Sample time for this block. It is the same meaning as general Simulink block .
Ports Input
• | StartAddr — "uint16" data type's scalar. It is "Simulated EEPROM" start address you want to write. This address is byte addressing.
• | Data — Scalar or Vector. It is data source for writing. Data type cannot be "logical", cannot be "double".
Outport
• | OK — "logical" data type's scalar. True means "Simulated EEPROM" address range you write is valid. Writing data success.
Examples