resetDevice | Top

resetDevice reset Modbus Server all register values Since R2019b Library: Modbus Server ( Dafulai Electronics) /resetDevice Description This block resets all register values to zero or false. Parameters Please double click this block to open parameters dialog below: Let us explain parameters.
• | Object ID for multiple Modbus slave Simulator Hardware — In one PC, we may use multiple Modbus slave simulators, this is for identifying each one.
• | Which device? (Only for RTU/ASCii) — This is useful only for Modbus RTU/ASCii Server. it denotes which device we want to reset. For Modbus TCP Server, just ignore it.
Ports Input
• | Reset — "logical" data type's scalar. Rising Edge from false to true causes "Reset registers to zero or false Action".
Outport
• | Success — "logical" data type's scalar. If succeed to reset, it will become true, otherwise false.