refresh | Top

refresh refresh CAN bus receiver buffers Since R2019b Library: CAN Bus Controller ( Dafulai Electronics) /refresh Description This block will refresh CAN Bus receiver buffers. After you executing this block, the previous CAN bus receiver information will disappear. Usually, we don't use this block because our CAN_setup block can set up "Auto-refresh" enabled. We use this block when "Auto-refresh" disabled. Parameters Please double click this block to open parameters dialog below: Let us explain parameters.
• | Object ID for multiple CAN Bus controllers — In one PC, we may use multiple CAN bus controllers, this is for identifying each one we use. It must match the same parameter in CAN_setup block.
Ports Input En — "number" scalar or "logical" scalar. true or >0 will make once refresh in this sampling time. Outport None