AllWriteReadDone | Top Next

AllWriteReadDone Are embedded Modbus Master all operations done? Since R2019b Library: embeddedCreatorLib ( Dafulai Electronics) / emModbus Master / AllWriteReadDone Description This block is used in judgment whether embedded Modbus master has done all reading/writing operations to all related Modbus Servers. In order to start new group of modbus operations, you must set Modbus master into "Idle" state when embedded target found this block output port "Yes" is true. Parameters
• | Sample time in sec (-1 for inherited): — Sample time for this block. It is the same meaning as general Simulink block .
Ports Input None Outport
• | Yes — "logical" data type's scalar. True means "embedded Modbus master has done all reading/writing operations to modbus servers. False means "embedded Modbus master has not done all reading/writing operations to modbus servers, it is busy to read / write servers.
Examples