emReset | Top

emReset Reset Target Micro-Controller Since R2019b Library: embeddedCreatorLib ( Dafulai Electronics) / emReset Description This block resets Target CPU and all peripherals. Notes: You can add only - one embedded Modbus Master or Client. You cannot create 2 or 2+ Modbus Masters or Clients. Parameters None But when you double click this block, you can open operation dialog below: "Reset" is command Button. When you click "Reset" Button during simulink running, A popup window occurs below: If you click "Yes", it will send "Reset" command to target, otherwise, cancel "Reset" command. If "Reset" success, it will display window below: If "Reset" failed, it will display window below: Ports Input None Outport None