emProbe | Top Next

emProbe embedded Probe. Since R2019b Library: embeddedCreatorLib ( Dafulai Electronics) / Modbus Slave & Debugger / emProbe Description This block will watch Simulink signal. Input Port connects Signal you want to watch. Output Port connects block "Display" to display signal values Notes: 1 Not all signals need "emProbe" to watch. For signal from port with ""Right Arrow" (à) symbol, you can directly connect block "Display" to watch them. 2 You can use block "Mux" to collect multiple signals, and then use one "emProbe" to watch. This way can save communication traffic, and all signals values are simultaneous. Parameters None Ports Input
• | — Any data type's scalar or vector. You connect it to any Simulink Signal you want to watch.
Outport
• | — The same as input port's signal. It connects block "Display" to watch signal values.
Examples